Specifications

Main Hardware System

number of channels | 5,9,13,16
Resolution | 16 bits on all channels.
Sample rate | variable. Maximum 22000 Hz for acoustics channel and 11000 Hz on other, depending on number of channels.
Filter Rate | Variable, depending on the sample rate.
Gain | variable on all channels
Input type | Acoustics channel, microphone and line. Other channels, mini-din, mini jacks, 15 pin VGA connector.
Input level | All channels +/- 2.5 volts with 10K input impedance.
Output type | Acoustics, phone and line. No other channels output is available.
Output level | Acoustics, +/- 1.25 volt line level.
Adjustment | All software controlled.
Host connection | USB
Platform | WIN98/98, 2000, XP and Mac OS X with USB support.
Power | 110/220 VAC universal input with 500 ma.
Size | 10"X7"X3"
Battery Option | 12V NICAD rechargeable, with up to 2 hours of operation under full load.

Transducer Interface System

Transducers | up to two flows and two pressures.
Signal deflection | Air into the transducers produce positive deflection and vice-versa.
Microphone | Electret, internally powered cartridge, with flat frequency response up to 10 Khz.
Power | +/- 5 volt supplied by the main hardware system.
Connector | Mini-Din.