Calibration...

The data calibration is perform on the basis a cubic polynomial whose coefficients are provided by the desire calibration function. In general one always uses a linear calibrating factor which only has a "D" value with everything else zero. Deviation from this should only be done by very "experienced users", as undesirable result may occur.

The table rows count will vary depending on the number of data channels present in the file.

Row title Shows the channel and its designation. (not editable).

Signal name Represents the name of the signal which you wish to give to your data.

A Coefficient for cubic term.

B Coefficient for quadratic term.

C Coefficient for linear term.

D Intercept.

Unit The conversion unit.