Smooth

This is running average of the values over a given window for all non-acoustics data channels. No smoothing is done for acoustics data channel. This is a simple filtering tool for obtaining the envelope. The default size is set to 5 points. Subsequent smoothing will result in smoothing the already smoothed data.

Please refer to the Intensity/Smooth Option dialog for setting the parameters.