Modify...

Main display

The software will launch a blank window. On the left side of the graphic display a series of displays shows the channel numbers along with the labels that you wish to provide for the signal on that channel, the amplitudes in desired units and the corresponding gain selection for that channel when it was recorded.

The cursor position and the duration of the selection are shown at the bottom of the screen in milliseconds.

Moving the mouse while holding the mouse button down makes the selection.

The marker is a specific location in time for performing FFT/LPC analysis and/or editing. To place a marker, move the cursor to the desire location and press the mouse button. The marker will be placed with a different color. Placing a new marker will remove the old marker.

The graphs for each channel can be moved up or down and the display gain (see note below) can be increased/decreased using the parameters in the display options.

The colors for all the displays can be altered with the display/color options.

The intensity values will display with a different color.

The graph window can zoom in and out using the zoom menu commands.