Log...

The data logging follows settings in this dialog.

Step Size for Selection , refers to the interval steps taken when you try to enter the actual data in each channel shown in the log file. Be careful as not to select a very small interval, then the log file becomes enormous.

Step Size for entire frame, refers to the step size taken when you enter the entire FFT/LPC frame into the log file.